wlan-decoder-java 1.0

- Main Page
- Packages
- Classes

- Class List
- Class Index
- Class Hierarchy
- Class Members

All Classes Namespaces Functions Variables Pages
Public Member Functions | List of all members
fr.bmartel.protocol.wlan.frame.management.element.subelement.inter.IMcsSupportedSet Interface Reference
Inheritance diagram for fr.bmartel.protocol.wlan.frame.management.element.subelement.inter.IMcsSupportedSet:
[legend]

## Public Member Functions
byte[] | getRxMcsBitmask ()
List< IWlanMcs > | getMcsList ()

## Detailed Description

parse MCS supported set subtype element

- RX MCS bitmask : b0-b76
- reserved : b77-b79
- RX Highest Supported Data Rate : b80-b89
- reserved : b90-b95
- TX MCS set defined : b96
- TX RX MCS set not equal : b97
- TX maximum number spatial streams supported : b98-b99
- TX unequal modulation supported : b100
- reserved : b101:b127

Author
  Bertrand Martel

The documentation for this interface was generated from the following file:

- /home/abathur/Bureau/wlandecoder/wlandecoder/src/fr/bmartel/protocol/wlan/frame/management/element/subelement/inter/IMcsSupportedSet.java