wlan-decoder-java 1.0

- Main Page
- Packages
- Classes

- Class List
- Class Index
- Class Hierarchy
- Class Members

All Classes Namespaces Functions Variables Pages
Public Member Functions | List of all members
fr.bmartel.protocol.wlan.frame.management.element.inter.ISsidElement Interface Reference
Inheritance diagram for fr.bmartel.protocol.wlan.frame.management.element.inter.ISsidElement:
[legend]

## Public Member Functions
String | getSsid ()

## Detailed Description

SSID element indicates the identity of an ESS or IBSS.

- element id : 1 Byte
- length : 1 Byte
- ssid : 0-32 Bytes

The length of the SSID field is between 0 and 32 octets. A SSID field of length 0 is used within Probe Request management frames to indicate the wildcard SSID. The wildcard SSID is also used in Beacon and Probe Response frames transmitted by mesh STAs

Author
  Bertrand Martel

The documentation for this interface was generated from the following file:

- /home/abathur/Bureau/wlandecoder/wlandecoder/src/fr/bmartel/protocol/wlan/frame/management/element/inter/ISsidElement.java