wlan-decoder-java 1.0

- Main Page
- Packages
- Classes

- Class List
- Class Index
- Class Hierarchy
- Class Members

All Classes Namespaces Functions Variables Pages
Public Member Functions | List of all members
fr.bmartel.protocol.wlan.frame.management.element.inter.ITimElement Interface Reference
Inheritance diagram for fr.bmartel.protocol.wlan.frame.management.element.inter.ITimElement:
[legend]

## Public Member Functions
byte | getDTIMcount ()
byte | getDTIMperiod ()
byte | getBitmapControl ()
byte[] | getPartialVirtualBitmap ()

## Detailed Description

Traffic indication message

A delivery traffic indication message is a frame that wake up sleeping wifi device to listen to router message

- element id : 1 byte
- length : 1 byte
- DTIM Count : number of beacon frame will appear before the next DTIM
- DTIM Period : number of beacon intervals between 2 DTIM
- Bitmap Control
- Partial Virtual Bitmap

Author
  Bertrand Martel

The documentation for this interface was generated from the following file:

- /home/abathur/Bureau/wlandecoder/wlandecoder/src/fr/bmartel/protocol/wlan/frame/management/element/inter/ITimElement.java